**Oviphone Technology Limited Company: W300G-4G-CAT1 device TCP protocol**

**The server needs to respond with F0 login packet (with specific response format) and F9 heartbeat packet (no specific response format), otherwise itl.**

Catalogue

[1. Overview 1](#_Toc191)

[2. Protocol Data Packet Structure 1](#_Toc24808)

[2.1. Data Header 1](#_Toc15202)

[2.2. Message ID 2](#_Toc839)

[2.3. Token Generation Mechanism 2](#_Toc3343)

[2.4. Payload 2](#_Toc21761)

[2.5. Checksum 3](#_Toc28726)

[3.messages 4](#_Toc7331)

[3.1 Connection related 4](#_Toc22441)

[3.1.1 LNK-LIN (0xF0) Request Connection (TCP Only) 4](#_Toc30307)

[3.1.2LNK-RPL(0xF1) Connection Reply (TCP only) - Important 5](#_Toc14533)

[3.1.3New heartbeat packet protocol (0xF9) - Important 6](#_Toc11295)

[3.1.4Heartbeat protocol (0xF6) (used in previous devices, will not coexist with F9) 7](#_Toc8190)

[3.2 Positioning related reporting 8](#_Toc8775)

[3.2.1GPS/BDS Position Reporting: Location Data Reporting (0x03) 8](#_Toc27308)

[3.2.2Upload of Wi-Fi and base station information (0xA4 improved version) 10](#_Toc10478)

[3.2.3 Bluetooth positioning information(LBE Location)（MsgId=0xD6） 12](#_Toc22596)

[3.3：Alarm related reporting 14](#_Toc15007)

[3.3.1Alarm data upload (0x02) 14](#_Toc30312)

[3.3.2Alarm data upload(0x21) (supplement to 0x02) 17](#_Toc16044)

[3.3.3upload alarm information（0x16） 18](#_Toc18038)

[3.4Equipment information and status reporting 18](#_Toc21255)

[3.4.1Status parameter reporting (MSGID=0xA9) - no need for parsing 19](#_Toc12406)

[3.4.2 Upload of software version and model（0XBB）- no need for parsing 19](#_Toc497)

[3.4.3 ICCID upload of SIM card (0xF3) 20](#_Toc13980)

[3.4.4Device charging status upload (0xC3)--Special version to use 21](#_Toc10745)

[3.5 Downstream feedback report 21](#_Toc13752)

[3.5.1Downlink feedback(MSGID=0xC0) 21](#_Toc21285)

[3.5.2Message status reporting(MSGID=0x28) 22](#_Toc8780)

[3.6Health related reports 23](#_Toc16960)

[3.6.1Health Data (MSGID = 0 x 32) 23](#_Toc28443)

[3.6.2Upload of device sleep analysis data (0xC5) 25](#_Toc25494)

[3.6.3Multiple Temperature Upload (0XBA) 26](#_Toc29041)

[3.6.4 Upload of device blood oxygen data(0xC6) 27](#_Toc12463)

[3.6.5Upload heart rate and blood pressure.(0xC2) 28](#_Toc30839)

[4.Setting 29](#_Toc4295)

[4.1Downlink 29](#_Toc14411)

[4.1.1 Set periodic upload（0x17） 29](#_Toc29202)

[4.1.2Message Send（MSGID=0X28） 31](#_Toc28343)

[4.1.3Setting（0XCE）---See detailed instructions-Important Downside 32](#_Toc2572)

[4.1.4 Domain Name Setting (0xC3) (TCP specific) 34](#_Toc5815)

[4.1.5 Issuance of dwell alarm trigger time（MSGID=0XCC） 35](#_Toc23909)

[4.1.6 Shutdown and restart (0x77) (issued when the device is turned on, this command is invalid when the device is turned off) 36](#_Toc26937)

[4.1.7Weather warning（0XCB） 36](#_Toc29779)

[4.1.8Personal information issued（0xCA） 39](#_Toc7345)

[4.1.9 Issue SOS prompt message (MSGID = 0 X 80) - -universal version firmware is not available, special firmware support 40](#_Toc1604)

[4.1.10 Issue message cleaning time (MSGID = 0 X 2 A) - -universal version firmware is not available, special firmware support 40](#_Toc8824)

[4.1.11Set the reporting period of health data sampling（MSGID=0X1C） 41](#_Toc69)

[4.1.12restore factory setting（MSGID=0X7B） 42](#_Toc22551)

# 

# Overview

This agreement is applicable to Oviphone Communication's W300G 4G CAT1 equipment, which currently supports products such as W300G .

* Use 32-bit data headers for synchronization and terminal identification;
* Implement verification protection using low-cost verification algorithms;
* Use message identifiers to indicate different messages.
* Unless otherwise specified. All applicable.

# Protocol Data Packet Structure

A basic protocol data packet structure is shown in Figure 1.：



**Figure1**

## Data Header

Each data packet begins with a 4-byte Header or token (in some response messages, a timestamp is used instead):

Currently, the token for Eurofins devices is fixed as BD BDBDBD

Header: 0xBD 0xBD 0xBD 0xBD

Timestamp: 32 bits, generated by the server

## Message ID

MessageId represents the content as described in Chapter 3.

Every time the TCP connection is established, the device side will first report the 0xF0 message, which contains the unique identifier IMEI of the device. The server side needs to record this IMEI as an identifier. Then it will respond with the 0xF1 message. The device side will consider the connection successful only after receiving this response. Otherwise, it will disconnect the link.

## Token Generation Mechanism

Currently fixed to BDBDBDBD

## Payload

The payload below refers to the effective content of the protocol, excluding the head token and checksum. The length of the content is indicated afterwards.

The data formats used in the payload are shown in the following table:

[U-unsigned; I-signed; X-bitfield; number-bytes occupied]

In the protocol below, little-endian is used for all data types except for ch, u8, i8, and x8.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Short** | **peTypeType** | **Size(Bytes)** | **Min/max** | **Resolution** | **explain** |
| CH | ASCII/ISO 8859.1 | 1 | - | - | char |
| u8 | Unsigned Char | 1 | 0..255 | 1 | unsigned short |
| i8 | Signed Char | 1 | -128..127 | 1 | short |
| x8 | Bitfield | 1 | - | - | bit |
| u16 | Unsigned Short | 2 | 0..65，535 | 1 | unsigned int |
| i16 | Unsigned Short | 2 | -32,768..32,767 | 1 | int |
| x16 | Bitfield | 2 | - | - | （bit）2 |
| u32 | Unsigned Long | 4 | 0..4,294,967,295 | 1 | unsigned long |
| i32 | Signed Long | 4 | -2,147,483,648..2,147,483,647 | 1 | long |
| u64 | Uint64\_t | 8 | 0..18,446,744,073,709,551,616 | 1 | uint64\_t |
| float | float | 4 | -3.44\*10e38..3.4\*10e38 | - | float |

## Checksum

The content to be added to the checksum includes the payload, as shown in Figure 1. The algorithm is as follows, where Buffer[N] represents the data to be accumulated.

Ck\_sum = 0

For(i=0; i<N; i++)

{

ck\_sum = ck\_sum + Buffer[i]

ck\_sum = ck\_sum % 0x100

}

ck\_sum = 0xFF – ck\_sum

Return ck\_sum

Where ck\_sum cannot exceed 0xFF, so after each loop, it must be modulo 0x100 and then taken the remainder.

# **3.**messages

## Connection related

### LNK-LIN (0xF0) Request Connection (TCP Only)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | LNK-LIN | | | |
| Description | Terminal requests to log into the terminal server through IMEI number | | | |
| Firmware |  | | | |
| Direction | Terminal => Terminal Server | | | |
| Payload length | 10bytes | | | |
| Message structure | Header | Message ID | Payload | Checksum |
| 0xBD 0xBD 0xBD 0xBD | 0xF0 | See below | CK\_sum |

Payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Byte Offset | Format | Name | Scale | Unit | Drscription |
| 8 | u64 | IMEI | 1 | - | IMEI number（little-endian） |
| 2 | x16 | version |  | - | Bitfield see below |
|  |  |  |  |  |  |

This request must have a response of 0xF1, otherwise the login will fail.

例：bdbdbdbdf09b51731bc6160300000014 （imei:869465050010011）

BDBDBDBD：4-byte message header

F0：Message ID

9b51731bc6160300：imei number (Little-endian mode)，imei decimal is 869465050010011，In hexadecimal, it is0x000316C6 1B73 519B, Little-endian mode:9b51731bc6160300

0000：version

14：checksum

When TCP creates a new connection, it first reports an F0 request, which includes the IMEI. The server then records this IMEI, and all the data in this connection will be associated with this IMEI.

### 3.1.2LNK-RPL(0xF1) Connection Reply (TCP only) - Important

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | LNK-RPL | | | |
| Description |  | | | |
| Firmware |  | | | |
| Direction | Terminal <= Terminal Server | | | |
| Payload length | 4 bytes | | | |
| Message structure | Header | Message ID | Payload | Checksum |
| Timestamp(unix) | 0xF1 | See below | CK\_sum |

Payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Byte Offset | Format | Name | Scale | Unit | Drscription |
| 4 | u32 | Token | 1 | - | Token:BDBDBDBD |

eg：28D4DE55F1BDBDBDBDEB

The response must be replied on the current channel. The first 4 bytes are the timestamp, and the device side synchronizes the time based on this, so it must be the correct timestamp value in little-endian mode. The reply is sent byte by byte, for example, BD counts as one byte.

The timestamp refers to the number of seconds or milliseconds from the current time to 1970-1-1 0:00. Milliseconds are easier to convert in Java. Our protocol uses seconds, so it's a long integer. We use little-endian preference, so it becomes the following format: 28D4DE55 --> 55 DE D4 28 is the actual value, and then this value is converted to a long integer. Adding this value to 1970-1-1 0:00 gives the current time.

Example: Timestamp = 07FD8860 real value 6088FD07 = 1619590407 seconds. This is 1619590407 seconds from 1970-01-01 00:00:00, which is the time reported by the device: 2021/4/28 6:13:27.

### 3.1.3New heartbeat packet protocol (0xF9) - Important

After the terminal connects to the server, it uploads a heartbeat packet to the server at fixed intervals.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_HTB\_UPL | | | |
| Decription | heartbeat packet | | | |
| Firmware | -/- | | | |
| Payload Length | 15 bytes | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0xF9 | 见下方定义 | CK\_sum |

payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Byte offset | Format | Name | Scale | Unit | Decription |
| 1 | U8 | Bat\_type |  |  | Battery Type  0: 4-level  1: 5-level  2: Percentage  3: Voltage |
| 2 | u16 | Bat\_volt |  | -/- | Battery Level  If Bat\_type is 0:  The battery level ranges from 0 to 3  (0 for 25%, 3 for 100%)  If Bat\_type is 1:  The battery level ranges from 0 to 4  (0 for 20%, 4 for 100%)  If Bat\_type is 2:  The battery level ranges from 0 to 100 |
| 1 | U8 | Signal\_type |  |  | Signal Type  0: Percentage  1: 5-level  2: CSQ value |
| 2 | I16 | Signal\_strength |  |  | Signal\_strength |
| 1 | U8 | Other\_type |  |  | Extension Type  0: Full Step Count  1: Incremental Step Count  2: Vibration |
| 4 | U32 | Num |  |  | Extended value |
| 4 | U32 | Timestamp | -/- | -/- | Utc Timestamp |

Heartbeat packets must be replied to,The device will consider the connection still exists as long as it receives a reply.

Reply example (can be fixed reply to this): BDBDBDBDF301

### 3.1.4Heartbeat protocol (0xF6) (used in previous devices, will not coexist with F9)

After the terminal connects to the server, it will upload a heartbeat packet to the server at regular intervals. The later versions will also include a timestamp.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_HTB\_UPL | | | |
| Decription | heartbeat packet | | | |
| Firmware | -/- | | | |
| Payload Length | 11 bytes | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0xF6 | See below | CK\_sum |

payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Byte offset | Format | Name | Scale | Unit | Decription |
| 2 | U16 | Bat\_volt |  | -/- | The number of battery power bars. |
| 4 | U32 | Step\_num |  |  | Step count data |
| 1 | U8 | Signal\_strength |  |  | Signal strength |
| 4 | U32 | Timestamp |  |  | timestamp (a timestamp will be added at the end when making up for missing data) |

eg：BDBDBDBDF6030000000000509C75FE6350

Bat\_volt=0 represents the battery percentage is 10%

Bat\_volt=1 represents the battery percentage is 30%

Bat\_volt=2 represents the battery percentage is 60%

Bat\_volt=3 represents the battery percentage is 100%

## 3.2 Positioning related reporting

### 3.2.1GPS/BDS Position Reporting: Location Data Reporting (0x03)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_UPL\_GPS | | | |
| Decription | 回馈GPS/BDS定位数据 | | | |
| Firmware | -/- | | | |
| Payload Length | 23 bytes | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0x03 | See below | CK\_sum |

payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Byte offset | Format | Name | Scale | Unit | Decription |
| 8 | Double | lon |  | -/- | longitude |
| 8 | Double | lat |  |  | latitude |
| 1 | U8 | north\_south |  |  | /\*N or S\*/ |
| 1 | U8 | east\_west |  |  | /\*E or W\*/ |
| 1 | U8 | status |  |  | /\*A or V\*/ |
| 4 | U32 | Timestamp |  |  | Timestamp |

Example： BDBDBDBD03000000C0424C5E4000000000A5DC3C404E4541E62C616078

Lon: 000000C0424C5E40Lat: 00000000A5DC3C40 4E –N 45-E 41-A Time E62C6160

Lon:121.191574Lat: 28.861893

Status = A indicates that the information content is accurate. It can be resolved to V and can be abandoned.

Example of GPS parsing (JAVA)：

DBDBDBDB037d9f84ac81815c40e766926b1d8936404e4541749d695f0b

//DBDBDBDB03 7d9f84ac81815c40 e766926b1d893640 4e 45 41 749d695f 0b

public static void main(String[] args){

//eg:7d9f84ac81815c40 -->405c8181ac849f7d

Double.longBitsToDouble(Long.parseLong("405c8181ac849f7d",16))); //114.02353966666665

//message e766926b1d893640 actual value 4036891d6b9266e7

Double.longBitsToDouble(Long.parseLong("4036891d6b9266e7", 16))) ;//22.535605166666667

HexToStr(data.Substring(“4e”)); //N

HexToStr(data.Substring(“45”));//E

HexToStr(data.Substring(“41”));//AA represents data "OK", V represents a warning

//Message 749d695f actual value 5f699d74

Date date=new Date();

date.setTime(Long.parseLong(“5f699d74",16)\*1000);

SimpleDateFormatsdf = new SimpleDateFormat("yyyyMMddHHmmss");

System.out.println(sdf.format(date)); //2020-09-22 14:45:08

### 3.2.2Upload of Wi-Fi and base station information (0xA4 improved version)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | EXT-CIU | | | |
| Description | Cell information upload.Upload cell tower information for terminal server to compute location. | | | |
| Firmware |  | | | |
| Direction | Terminal -> Terminal Server | | | |
| Payload length |  | | | |
| Message structure | Header | Message ID | Payload | Checksum |
| Token | 0xA4 | See below | CK\_sum |

Payload contents:

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Byte Offset** | **Format** | | **Name** | | **Scale** | | | **Unit** | | **Description** |
| 4 | U32 | | UtcTime | |  | | |  | | Search Time |
| 1 | u8 | | Cell\_cnt | | 1 | | | - | | Number of cell info payload.Valid value:1~7 |
| 2 | u16 | | Cell[0].MCC | | - | | | - | | mobile country code of cell[0] |
| 2 | u16 | | Cell[0].MNC | | - | | | - | | mobile network code of cell[0] |
| 2 | u16 | | Cell[0].LAC | | - | | | - | | Location area code of cell[0] |
| 4 | U32 | | Cell[0].CELL\_ID | | - | | | - | | Cell id of cell[0] |
| 2 | i16 | | Cell[0].RSSI | | - | | | dbm | | RSSI in dbm of cell[0] |
| … |  | |  | |  | | |  | |  |
| 2 | u16 | | Cell[cell\_cnt-1].LAC | | - | | | - | | Location area code of cell[[cell\_cnt-1] |
| 4 | U32 | | Cell[cell\_cnt-1].CELL\_ID | | - | | | - | | Cell id of cell[[cell\_cnt-1] |
| 2 | I16 | | Cell[cell\_cnt-1].RSSI | | - | | | dbm | | RSSI in dbm of cell[[cell\_cnt-1] |
| 1 | U8 | | Wifi\_cnt | |  | | |  | | Number 0f wifi |
| 1 | U8 | | Wifi[0].bssid[0] | |  | | |  | |  |
| 1 | U8 | | Wifi[0].bssid[1] | |  | | |  | |  |
| 1 | U8 | | Wifi[0].bssid[2] | |  | | |  | |  |
| 1 | U8 | | Wifi[0].bssid[3] | |  | | |  | |  |
| 1 | U8 | | Wifi[0].bssid[4] | |  | | |  | |  |
| 1 | U8 | | Wifi[0].bssid[5] | |  | | |  | |  |
| 4 | I32 | | Wifi[0].rssi | |  | | |  | |  |
|  |  | |  | |  | | |  | |  |
| 1 | U8 | | Wifi[Wifi\_cnt-1].bssid[0] | |  | | |  | |  |
| 1 | U8 | | Wifi[Wifi\_cnt-1].bssid[1] | |  | | |  | |  |
| 1 | U8 | | Wifi[Wifi\_cnt-1].bssid[2] | |  | | |  | |  |
| 1 | U8 | | Wifi[Wifi\_cnt-1].bssid[3] | |  | | |  | |  |
| 1 | U8 | | Wifi[Wifi\_cnt-1].bssid[4] | |  | | |  | |  |
| 1 | U8 | | Wifi[Wifi\_cnt].bssid[5] | |  | | |  | |  |
| 4 | | I32 | | Wifi[wifi\_cnt].rssi | |  |  | |  | |

Note: A total of 7 base station information will be provided, including the serving cell and the adjacent 6 cells.

Message ID:A4

BDBDBDBDA468984C5F01CC010000C21871F543009E00078CBEBE1A8162C6FFFFFFC061180AF42AC1FFFFFF200BC726E000B6FFFFFFA8154DF6517EB2FFFFFFE005C5B1F824CCFFFFFFE8FCAFA02663AFFFFFFF6409805B2B9CAEFFFFFF94

To finally obtain the latitude and longitude data, please refer to the relevant explanation in Section 4.4 of the "Explanation of WiFi positioning regarding protocol parsing for A3, A2, and A4"And amap wifi positioning protocol（It is currently only available in the Chinese version）



### 3.2.3 Bluetooth positioning information(LBE Location)（MsgId=0xD6）

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_HTB\_UPL | | | |
| Decription | LBE Location | | | |
| Firmware | -/- | | | |
| Payload Length | 1 bytes +n | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0xD6 | See below | checksum |

Payload:

|  |  |  |  |
| --- | --- | --- | --- |
| Format | Name | Scale | Description |
| U8 | Type | 1 | Currently fixed to0 (Fix value 0) |
| U8 | Total\_groups | 1 | Total number of assemblies, there may be multiple sets of information, and each set may contain multiple items.  ibeacon (The total number of groups, there may be multiple groups of information, and there may be multiple ibeacons in each group) |
| Int32 | Utc | 4 | Utctimestamp (the UTC timestamp of the first group) |
| U8 | Total\_PackCount | 1 | Total number of packages at the current time: (the ibeacon’s count of the first group) |
| U16 | Major0 | 2 | Major |
| U16 | Minor0 | 2 | Minor |
| S8 | Rssi0 | 1 | Rssi |
| U16 | MajorN | 2 | Major |
| U16 | MinorN | 2 | Minor |
| S8 | RssiN] | 1 | Rssi |
| Int32 | Utc | 4 | Utc timestamp (UTC timestamp of the second group) |
| U8 | Total\_PackCount | 1 | Total number of packages at the current time (the ibeacon’s count of current group) |
| U16 | Major0 | 2 | Major |
| U16 | Minor0 | 2 | Minor |
| S8 | Rssi0 | 1 | Rssi |
| U16 | MajorN | 2 | Major |
| U16 | MinorN | 2 | Minor |
| S8 | RssiN] | 1 | Rssi |

Example：

bdbdbdbdd60001be20315f0443271794ac43273094aa4327b956a54327fe94a56a

**bdbdbdbd - header**

**d6 - msgID**

**00 - type**

**01 -- Only one set of iBeacon data（total groups of beacons data :1）**

be20315f -- The first group’s timestamp: 0x5f3120be=1597055166

There are 4 beacon information in the first group.4327 --- major : 0x2743 = 10051

1794--- minor: 0x9417 = 37911

ac--- rssi: 0xac = -84

4327 --- major: 0x2743 = 10051

3094--- minor:0x9430 = 37936

aa--- rssi:-86

4327 --- major: 0x2743 = 10051

b956--- minor:0x56b9 = 22201

a5--- rssi:-91

4327 --- major: 0x2743 = 10051

fe94--- minor:0x94fe=38142

a5--- rssi:-91

6a --checksum

**3.3：Alarm related reporting**

### 3.3.1Alarm data upload (0x02)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | LNK-WRN | | | |
| Description | Terminal uploads its warnings to terminal server. | | | |
| Firmware |  | | | |
| Direction | Terminal => Terminal Server | | | |
| Payload length | 6 bytes | | | |
| Message structure | Header | Message ID | Payload | Checksum |
| Token | 0x02 | See below | CK\_sum |

Payload contents

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Byte Offset | Format | | Name | Scale | Unit | Drscription |
| 2 | x16 | | Upl\_warn | - | - | Bitfield see below(Little-endian) |
| 4 | | U32 | Timestamp |  |  | Timestamp (timestamp will be added afterwards for supplementary upload) |
|  |  | |  |  |  |  |

Bitfield WRN:

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 15 |  |  |  |  |  |  |  |  |  |  | 4 |  |  | 1 | 0 |

Below is the corresponding definition table for when the bit is 1 and the current alarm. Multiple alarms may also be present simultaneously.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| bit | Name | Description | Code | Adjusted hexadecimal | decimalism |
| 15 | Gas alarm（- special equipment support） | Gas alarm（- special equipment support） | 0 | 8000 |  |
| 14 | Drop the alarm | Drop the alarm | 1 | 4000 | 4\*4096=16384 |
| 13 | Fence alarm（- special equipment support） | Fence alarm (away from the beacon) （- special equipment support）） | 2 | 2000 | 2\*4096=8192 |
| 12 | Strap damage（- special equipment support） | Strap damage（- special equipment support） | 3 | 1000 | 1\*4096=4096 |
| 11 | Lock open（- special equipment support） | Lock open（- special equipment support） | 4 | 0800 | 8\*256=2048 |
| 10 | Approaching beacon point (125K) （- special equipment support） | Approaching beacon point (125K) （- special equipment support） | 5 | 0400 | 4\*256=1024 |
| 9 | Release key  （- special equipment support） |  | 6 | 0200 | 2\*256=512 |
| 8 | Wearing device | Wearing device | 7 | 0100 | 1\*256=256 |
| 7 | Cancel SOS | Cancel SOS | 8 | 0080 | 8\*16=128 |
| 6 | Vibration alarm（- special equipment support） | Vibration alarm（- special equipment support） | 9 | 0040 | 4\*16=64 |
| 5 | Sedentary alarm | Sedentary alarm | 10 | 0020 | 2\*16=32 |
| 4 | Remove device | Remove device | 11 | 0010 | 1\*16=16 |
| 3 | Open box alarm（- special equipment support） | Open box alarm（- special equipment support） | 12 | 0008 | 8 |
| 2 | Shutdown | Shutdown | 13 | 0004 | 4 |
| 1 | SOS |  | 14 | 0002 | 2 |
| 0 | Low Battery | Low Battery | 15 | 0001 | 1 |

BDBDBDBD02020007FD8860E7 true value 0002—0000 0000 0000 0010 SOS alarm

Timestamp = 07FD8860 is equal to 6088FD07 = 1619590407. This represents the time when 1619590407 seconds have elapsed since 1970-01-01 00:00:00. This corresponds to the device reporting the time as 2021/4/28 6:13:27.

Alarm 02 and each independent, the status of the corresponding bit is not associated in the context of non-related alarms, only the current bit alarm with a value of 1 is processed, and the corresponding processing is performed.

### 3.3.2Alarm data upload(0x21) (supplement to 0x02)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | LNK-WRN | | | |
| Description | Terminal uploads its warnings to terminal server. | | | |
| Firmware |  | | | |
| Direction | Terminal => Terminal Server | | | |
| Payload length | 8 bytes | | | |
| Message structure | Header | Message ID | Payload | Checksum |
| Token | 0x21 | See below | CK\_sum |

Payload contents

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Byte Offset | Format | | Name | | Scale | Unit | Drscription | |
| 2 | U16 | | type | |  |  | Type of alarm | |
| 4 | U32 | | Upl\_warn | | - | - | Bitfield see below(Small end priority) | |
| 4 | U32 | Timestamp | |  | |  | | Timestamp (timestamp will be added afterwards for supplementary upload) |
|  |  | |  | |  |  |  | |

Alarm type =1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 2 | Device is charging and powered off (firmware functionality support required) |  | 29 | 0004 | 4 |
| 1 | Device low on power, powered off (firmware functionality support required) |  | 30 | 0002 | 2 |
| 0 | Device powered off manually (firmware functionality support required) |  | 31 | 0001 | 1 |

BDBDBDBD21010001000000ECFFBE65DA

### 3.3.3upload alarm information（0x16）

Special Note: This is a supplement to 0x02. The original 0x02 is limited by the number of digits and cannot represent these combinations of alarms.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_NB\_SOS | | | |
| Decription | Upload SOS information, including temperature and heart rate alarms. | | | |
| Firmware | -/- | | | |
| Payload Length | 7+4 bytes | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0x16 | See below | CK\_sum |

payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Byte offset | Format | Name | Scale | Unit | Decription |
| 1 | U8 | Type | -/- | -/- | Alarm types (  0: heart rate alarm  1:temperature alarm) |
| 2 | U16 | Heart | -/- | -/- | heart rate |
| 2 | U16 | temperature | -/- | -/- | temperature |
| 2 | U16 | Pa | -/- | -/- | pressure |
| 4 | 4\*U8 or U32 | expand | -/- | -/- | 4-byte extension for other sensors. |

Currently, the last four bytes of the isolated wristband are used as a timestamp.

**3.4Equipment information and status reporting**

### 3.4.1Status parameter reporting (MSGID=0xA9) - no need for parsing

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_HRD\_DATA | | | |
| Decription | Terminal => Server | | | |
| Firmware | -/- | | | |
| Payload Length | 6 bytes | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0xA9 | See below | CK\_sum |

1. payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Byte offset | Format | Name | Scale | Unit | Decription |
| 1 | u8 | TypeCnt | -/- | -/- | Type number |
|  |  |  |  |  | (Reserved 00） |
| 1 | u8 | Type | -/- | -/- | Type 1 |
| 1 | U8 | NameLen | -/- | -/- | Type1 length |
| n | N\*u8 | Name | -/- | -/- | name |
| 1 | u8 | Type | -/- | -/- | Type 2 |
| 1 | U8 | NameLen | -/- | -/- | Type 2 length |
| n | N\*u8 | Name | -/- | -/- | name |
|  |  |  |  |  |  |

Report one message upon startup

Type specified screen system (MCU module sensor wifi screen Bluetooth)

Code MCU 00 module 01 sensor 02 sequentially expands

Name lengthBDBDBDBDA9 01 00 00---mcu

125732303050475F4534322E57472E4D4C3238C8

### 3.4.2 Upload of software version and model（0XBB）- no need for parsing

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_VERSION\_DATA | | | |
| Decription | Upload of software version and model，Terminal=>Terminal Server | | | |
| Firmware | -/- | | | |
| Payload Length | 2+N bytes | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0xBB | See below | CK\_sum |

payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Byte offset | Format | Name | Scale | Unit | Decription |
| 1 | UINT8 | Version\_len | Required | / | The length of the software version number |
| N | S8[n] |  | Required |  | Software Version Number |
| 1 | UINT8 | Model\_len | Optional |  | Model length |
| N | S8[n] |  | Optional |  | Model Number |
| expandable |  |  |  |  | expandable |
|  |  |  |  |  |  |

Note: Previous firmware version used, now do reserved

### 3.4.3 ICCID upload of SIM card (0xF3)

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Message | | | LNK-LIN | | | | | | |
| Description | | | The terminal reports iccid to the server .when it logs on first | | | | | | |
| Firmware | | |  | | | | | | |
| Direction | | | Terminal => Terminal Server | | | | | | |
| Payload length | | | 10bytes | | | | | | |
| Message structure | | | Header | | | Message ID | | Payload | Checksum |
| 0xBD 0xBD0xBD0xBD | | | 0xF3 | | See below | CK\_sum |
| Byte Offset | Format | Name | | Scale | Unit | | Drscription | | | |
| 10 | 10\*U8 | ICCID | | 1 | - | | ICCID number | | | |

iccid:89861118236001639994

message :BDBDBDBDF389861118236001639994CC

Note:Start up and report

### 3.4.4Device charging status upload (0xC3)--Special version to use

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_HRD\_DATA | | | |
| Decription | Device charging status upload ，Terminal=>Terminal Server | | | |
| Firmware | -/- | | | |
| Payload Length | 5 bytes | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0xC3 | See below | CK\_sum |

payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Byte offset | Format | Name | Scale | Unit | Decription |
| 0 | U8 | Status | / | / | 0start，  1end，  2 fully charged |
| 1 | U32 | Timestamp |  |  | Timestamp |

Eg:

BDBDBDBDC301DB4D2F668A The device is charged at the end

BDBDBDBDC300DB4D2F668A The device starts charging

BDBDBDBDC302DB4D2F668A The equipment is fully charged

**3.5 Downstream feedback report**

### 3.5.1Downlink feedback(MSGID=0xC0)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_HRD\_DATA | | | |
| Decription | Terminal =>Server | | | |
| Firmware | -/- | | | |
| Payload Length | 1 +n bytes | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0xC0 | See below | CK\_sum |

payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Byte offset | Format | Name | Scale | Unit | Decription |
| 1 | U8 | length | -/- |  | Message IDlength |
| N | n\*U8 | type | -/- |  | N Message ID |
|  |  |  |  |  |  |

This command is used for the feedback of downlink commands, returning the Message ID(s) received earlier (multiple Message ID can be returned collectively).

### 3.5.2Message status reporting(MSGID=0x28)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_HRD\_DATA | | | |
| Decription | Terminal =>Server | | | |
| Firmware | -/- | | | |
| Payload Length | 1 bytes | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0x28 | See below | CK\_sum |

payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Bytes | Format | Name | Scale | Unit | Decription |
| 4 | U32 | timestamp | -/- | -/- | Time stamp |
| 1 | U8 | type | -/- | -/- | Type (corresponding to 0X28 downlink), currently 0x03 |
| 1 | U8 | status | -/- | -/- | Message status  1: Read, received |
| 4 | U32 | serial number | -/- | -/- | (corresponding to 0X28 downlink) |
|  |  |  |  |  |  |

## 3.6Health related reports

### 3.6.1Health Data (MSGID = 0 x 32)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. Message | MSG\_HRD\_DATA | | | |
| Decription | Heart rate data upload，Terminal=>Terminal Server | | | |
| Firmware | -/- | | | |
| Payload Length | 8+3n bytes | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0x32 | See below | CK\_sum |

payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Byte offset | Format | Name | Scale | Unit | Decription |
| 1 | U8 | Type |  |  | 00 |
| 4 | U32 | Timestamp |  |  | Time stamp |
| 2 | U16 | contentLength |  |  | the total length of the following content |
| 1 | U8 | ID |  |  | ID (Type (5) + Reported Value Length (3)) |
| 2 | U16 | Val1 |  |  | Reported value of ID |
|  |  |  |  |  |  |
| 1 | U8 | ID |  |  | ID (Type (5) + Reported Value Length (3)) |
| 2 | U16 | Val1 |  |  | Reported value of IDn |

BDBDBDBD32 00 7A 89 0F 60 06 00 0A 32 10 12 04 00 03

The timestamp in the protocol is 7A 89 0F 60, type 00 mixed type single data reported content full length 06 00.

The ID is 0A, where 0A corresponds to 00001010 00001 010 (the first 5 bits are 01, and the following represent a reported length of 2 bytes). The last 2 digits behind the step count represent the number of steps.

The ID codes are as follows (the protocol defines the high 5 bits of the ID):

01 Step count

02 Heart rate

03 Body temperature

04 Wrist temperature

05 Blood sugar

06 Diastolic pressure

07 Systolic pressure

08 Blood oxygen

10 Number of sit-ups

11 Running pace and distance

12 Skipping speed and count

Eg1:

BDBDBDBD3200B3C4F2630F000A1E00114B314A39711A4A0122bc00416212

B3C4F263: 63f2c4b3(Hexadecimal timestamp)

0F00 :Total length excluding the last byte (checksum)

0A1E00：0x0A=00001 010. The first five bits are 00001, representing the data ID for step counting (0x01). The last three bits are 010, indicating that the length of the step count data is 2 bytes. 0x001E represents step count data, totaling 30 steps.

114B：0x11=00010001. The first five bits are 00010, representing the data ID for heart rate (0x02). The last three bits are 001, indicating that the length of the heart rate data is 1 byte. 0x4B represents the heart rate data, with a heart rate of 75.

314A：0x31=00110001. The first five bits are 00110, representing the data ID for diastolic blood pressure (0x06). The last three bits are 001, indicating that the length of the diastolic blood pressure data is 1 byte. 0x4A represents the diastolic blood pressure data, which is 74.

3971：0x39=00111 001. The first five bits are 00111, representing the data ID for systolic blood pressure (0x07). The last three bits are 001, indicating that the length of the systolic blood pressure data is 1 byte. 0x71 represents the systolic blood pressure data, which is 113.

1A4A01：0x1A=00011 010. The first five bits are 00011, representing the data ID for temperature (0x03). The last three bits are 010, indicating that the length of the temperature data is 2 bytes. 0x014A represents the temperature data, which is 330.

22BC00 ：0x22=00100 010. The first five bits are 00100, representing the data ID for wrist temperature (0x04). The last three bits are 010, indicating that the length of the wrist temperature data is 2 bytes. 0x00BC represents the wrist temperature data, which is 188.

4162：0x41=01000001 The first five bits are 01000, code data id blood oxygen (0x08), the last three bits 001, represents the blood oxygen data length of 1 byte, 0x62 is blood oxygen data, 98

### 3.6.2Upload of device sleep analysis data (0xC5)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_HTB\_UPL | | | |
| Decription | AnalyseSlepp Data；Report time: 21:00-08:00 | | | |
| Firmware | -/- | | | |
| Payload Length | 14 bytes | | | |
| Message structure | Hearer | Message ID | Payload |  |
| token | 0xC5 | See below | -/- |

payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Byte offset | Format | Name | Scale | Unit | Decription |
| 4 | Int32 | DateTime |  | -/- | Upload UTC start time |
| 4 | Int32 | DateTime |  |  | Upload UTC end time |
| 2 | Int16 | Sleepminute |  |  | Upload minutes of sleep time |
| 4 | Int32 | Type |  |  | Upload type, 1 for deep sleep, 2 for light sleep, 3 for awake duration |
|  |  |  |  |  |  |

BDBDBDBDC5AC338860693B8860210001000000D1

It indicates 1 for deep sleep, start time 2021/4/27 23:54:20, end time 2021/4/28 0:27:21, duration 33 minutes.

### 3.6.3Multiple Temperature Upload (0XBA)

**---Previously used by the device, the current health data is 0x32**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_TEMP\_DATA | | | |
| Decription | Multiple Temperature Upload ，Terminal=>Terminal Server | | | |
| Firmware | -/- | | | |
| Payload Length | 12 bytes | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0xBA | See below | CK\_sum |

payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Byte size | Format | Name | Scale | Unit | Decription |
| 1 | U8 | Timestamp identifier | Required |  | 00 - with timestamp; 01 - without timestamp |
| 4 | Int32 | Timestamp | Optional |  | If the timestamp identifier is 01, this field is not required |
| 1 | U8 | Temperature type | Required |  | 1: Indicates the upload of body surface temperature and body temperature  2: Indicates the upload of body surface temperature, body temperature, and ambient temperature |
| 2 | S16 | Body surface temperature | Optional |  | Body surface temperature with one decimal point (×10), reported value is an integer. Whether this field is present depends on the temperature type. |
| 2 | S16 | Body temperature | Optional |  | Body temperature with one decimal point (×10), reported value is an integer. Whether this field is present depends on the temperature type. |
| 2 | S16 | Ambient temperature | Optional | / | Ambient temperature with one decimal point (×10), reported value is an integer. Whether this field is present depends on the temperature type. |

### 3.6.4 Upload of device blood oxygen data(0xC6)

**---Previously used by the device, the current health data is 0x32**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_HTB\_UPL | | | |
| Decription | Uuid | | | |
| Firmware | -/- | | | |
| Payload Length | 6 bytes | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0xC6 | See below | CK\_sum |

payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Byte offset | Format | Name | Scale | Unit | Decription |
| 2 | I16 | BloodOxygen |  | -/- | Upload blood oxygen |
| 4 | U32 | Timestamp |  |  | timestamp (a timestamp will be added at the end when making up for missing data) |

### 3.6.5Upload heart rate and blood pressure.(0xC2)

**---Previously used by the device, the current health data is 0x32**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_BP\_UPL | | | |
| Decription | Upload heart rate and blood pressure | | | |
| Firmware | -/- | | | |
| Payload Length | 10 bytes | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0xC2 | See below | CK\_sum |

payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Byte offset | Format | Name | Scale | Unit | Decription |
| 2 | U16 | bp\_high | - | - | Systolic pressure：2byte |
| 2 | U16 | bp\_low | - | - | Diastolic pressure：2byte |
| 2 | U16 | Bp\_heart | - | - | heart rate：2byte |
| 4 | U32 | Timestamp |  |  | timestamp (a timestamp will be added at the end when making up for missing data) |
|  |  |  |  |  |  |

BDBDBDBDC275004D004A007A890F60CB

Systolic pressure 00 75 =117 Diastolic pressure 00 4D = 77 heart rate 00 4A =66

# **4.Setting**

## 4.1Downlink

### Set periodic upload（0x17）

The platform sets 1-4 time slots to send to the terminal. After the terminal receives the data, it uploads the data within the specified time slot.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_NB\_SLT | | | |
| Decription | downlink | | | |
| Firmware | -/- | | | |
| Payload Length | 28 bytes | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0x17 | See below | CK\_sum |

payload contents

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Byte offset** | **Format** | **Name** | **Scale** | **Unit** | **Decription** |  |
| 1 | u8 | enable | -/- | -/- | Enabled? | Time Slot 1 |
| 1 | U16 | Interval |  |  | Time interval (minutes) |
| 1 | u8 | time\_start\_h |  |  | -h |
| 1 | u8 | time\_start\_m |  |  | -m |
| 1 | u8 | time\_end\_h |  |  | -h |
| 1 | u8 | time\_end\_m |  |  | -m |
| 1 | u8 | enable | -/- | -/- | Enabled? | Time Slot 2 |
| 1 | U16 | Interval |  |  | Time interval (minutes) |
| 1 | u8 | time\_start\_h |  |  | -h |
| 1 | u8 | time\_start\_m |  |  | -m |
| 1 | u8 | time\_end\_h |  |  | -h |
| 1 | u8 | time\_end\_m |  |  | -m |
| 1 | u8 | enable | -/- | -/- | Enabled? | Time Slot 3 |
| 1 | U16 | Interval |  |  | Time interval (minutes) |
| 1 | u8 | time\_start\_h |  |  | -h |
| 1 | u8 | time\_start\_m |  |  | -m |
| 1 | u8 | time\_end\_h |  |  | -h |
| 1 | u8 | time\_end\_m |  |  | -n |
| 1 | u8 | enable | -/- | -/- | Enabled? | Time Slot 4 |
| 1 | U16 | Interval |  |  | Time interval (minutes) |
| 1 | u8 | time\_start\_h |  |  | -h |
| 1 | u8 | time\_start\_m |  |  | -m |
| 1 | u8 | time\_end\_h |  |  | -h |
| 1 | u8 | time\_end\_m |  |  | -m |

Example：

bd bd bd bd 17 01 03 00 00 00 13 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 dd

From 0:00 to 19:00, location is updated every 3 minutes.

BDBDBDBD17010A000000173B00000000000000000000000000000000000000000097

From 0:00 to 23:59, location is updated every 10 minutes.

### 4.1.2Message Send（MSGID=0X28）

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_HRD\_DATA | | | |
| Decription | Server =>Terminal downlink | | | |
| Firmware | -/- | | | |
| Payload Length | 7+n bytes | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0x28 | See below | CK\_sum |

payload contents

|  |  |  |  |
| --- | --- | --- | --- |
| Byte size | Format | Name | Decription |
| 1 | U8 | type | (Message type, if it is downlink information, the fixed value is 03) |
| 4 | Uint32 | seqID | Information id, uniqueness |
| 1 | U8 | CONTENT LEN | Contect Length |
| N | N | CONTENT | content, Chinese is GB2312 code, English is ascii code |
|  |  |  |  |
|  |  |  |  |

Example：bd bd bd bd 28 03 03 00 00 00 0b 68 65 6c 6c 6f 2c 77 6f 72 6c 64dd

Type: 03

seqId:03 00 00 00

CONTENT LEN: 0b (10)

CONTENT :68 65 6c 6c 6f 2c 77 6f 72 6c 64 ( hello,world)

### 4.1.3Setting（0XCE）---See detailed instructions-Important Downside

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_HRD\_DATA | | | |
| Decription | setting，Server => Terminal downlink | | | |
| Firmware | -/- | | | |
| Payload Length | 4+n bytes | | | |
| Message structure | Header | Message ID | Payload | Checksum |
| token | 0xCE | See below | CK\_sum |

payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Byte offset | Format | Name | Scale | Unit | Decription |
| 0 | u8 | Type | -/- | -/- | Type see below |
| 1 | u8 | Valid | -/- | -/- | Temporary valid, always valid |
| 2 | U16 | Len | -/- | -/- | Length of the following instruction |
| 4 | n |  | -/- | -/- | Main text |
|  |  |  |  |  |  |

Type 01 Positioning 02 health 03 Alarm (not reserved yet) 04 Local storage (not reserved yet)

05Bluetooth radio switch 06Position and health data reporting switch 07 Fall alarm switch 08 Stay alarm switch, expandable at the back

Valid 00 Always valid 01 Effective this time 02 Off

Length Length of the following instruction

Main text:

Type

01 Positioning function The main text can only be the basic class 01 - gps 02 - wifi 03 - Bluetooth beacon 04 - LBS base station 05 - 125k and later expanded basic class The main text can be a combination of 01 or 010204;

Such as 010203 means using gps wifi Bluetooth beacon;

Example: wifi positioning priority (wifi> Bluetooth> gps): BDBDBDBDCE0100030002030133

gps positioning priority (gps> wifi> Bluetooth): BDBDBDBDCE0100030001020333

Bluetooth positioning priority (Bluetooth beacon deployment required, Bluetooth> wifi> gps): BDBDBDBDCE0100030003020133,

Analysis example: wifi positioning priority (wifi> Bluetooth> gps): BDBDBDBD CE 01 00 0300 020301 33

Type: 01; Valid: 00; length: 0300; type: 020301; checksum: 33

03 The local alarm function can set heart rate alarm, and the blood pressure alarm falls off. which can be expanded after falling (type definition to be added) - -reserved for no

04 Local storage function (reserved) Keep those data in time-reserved temporarily

05 Bluetooth radio switch

00---open eg:BDBDBDBDCE0500000093

02---close eg:BDBDBDBDCE0502000093

07 Fall alarm switch

00---open eg:BDBDBDBDCE0700000093

02---close eg:BDBDBDBDCE0702000093

08 Stay alarm switch

00---open eg:BDBDBDBDCE0800000093

02---close eg:BDBDBDBDCE0802000093

09 Data reporting switch (all, keep only the heartbeat packet for long connection)

00---open eg:BDBDBDBDCE0900000093

02---close eg:BDBDBDBDCE0902000093

10 Report the location information immediately

01---An effective eg:BDBDBDBDCE0A01000093

11 Report the health data immediately

01---An effective eg:BDBDBDBDCE0B01000093

### 4.1.4 Domain Name Setting (0xC3) (TCP specific)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_SET\_DOMAIN | | | |
| Decription | Domain name settings downstream | | | |
| Firmware | -/- | | | |
| Payload Length | 52 bytes | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0XC3 | See below | CK\_sum |

payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Byte offset | Format | Name | Scale | Unit | Decription |
| 1 | U8 | Type |  |  | Type of issuance |
| 2 | U16 | Port |  |  | Port number (2 bytes) |
| 1 | U8 | Length |  |  | Length |
| N | U8 | Domainname |  |  | Type=1 IPv4 specific  Type 2 IPV6 specific (ASCII encoding) - not currently supported  Type=3 domain specific  (ASCII encoding) |

explain：type =1 4byte 0F:12:34:4A

type=2 IPv6

Eg：BDBDBDBDC302792204 33

BDBDBDBD C3 01 7922 04 76B2B8DB 33

01 type=1 ipv4

1. --Turn the big end--2279 --》Convert to decimal port：8825

76B2B8DB --》Convert to decima 118.178.184.219

33 checksum

### 4.1.5 Issuance of dwell alarm trigger time（MSGID=0XCC）

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_HRD\_DATA | | | |
| Decription | Issuance of dwell alarm trigger time，Server => Terminal | | | |
| Firmware | -/- | | | |
| Payload Length | 4+n bytes | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0xCC | See below | CK\_sum |

payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Byte offset | Format | Name | Scale | Unit | Decription |
| 0 | U8 | minute | -/- | -/- | The duration of the stay alarm (unit: minutes; value range 2-60), during which no activity will trigger the stay alarm |

Example：

bd bd bd bd cc 05 dd

05 -- 0x05 Report a stop alarm for 5 consecutive minutes of inactivity on the watch (when the watch is worn)

### 4.1.6 Shutdown and restart (0x77) (issued when the device is turned on, this command is invalid when the device is turned off)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_CFG\_PWR | | | |
| Decription | Shutdown and restart （issued when the device is turned on, this command is invalid when the device is turned off） | | | |
| Firmware | -/- | | | |
| Payload Length | 1 bytes | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0x77 | See below | CK\_sum |

payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Byte offset | Format | Name | Scale | Unit | Decription |
| 1 | u8 | enable | -/- |  | 1shut down |
| 1 | u8 | enable | -/- |  | 0 restart |

Eg：

restart："BDBDBDBD770193"

shut down："BDBDBDBD770093"

### 4.1.7Weather warning（0XCB）

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_HRD\_DATA | | | |
| Decription | Server => Terminal down | | | |
| Firmware | -/- | | | |
| Payload Length | 4+n bytes | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0xCB | See below | CK\_sum |

payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Byte offset | Format | Name | Scale | Unit | Decription |
| 0 | U8 | Count | -/- | -/- | Several sets of weather warnings |
| 1 | U8 | type | -/- | -/- | Weather warning type |
| 1 | U8 | Status | -/- | -/- | status |
| … | … | ……. |  |  | ….. |

Type：

|  |  |  |  |
| --- | --- | --- | --- |
| Type | Decription | Status |  |
| 1 | Storm warning | 0 | Cancel the alarm |
| 1 - 8 |  |
| 2 | rainstorm warning | 0 | Cancel the alarm |
| 1 |  |
| 2 |  |
| 3 |  |
| 3 | Thunderstorm warning | 0 | Cancel the alarm |
| 1 |  |
| 4 | Flood warning | 0 | Cancel the alarm |
| 1 |  |
| 5 | Mountain mud pouring warning | 0 | Cancel the alarm |
| 1 |  |
| 6 | Strong monsoon warning | 0 | Cancel the alarm |
| 1 |  |
| 7 | Frost warning | 0 | Cancel the alarm |
| 1 |  |
| 8 | Fire danger warning | 0 | Cancel the alarm |
| 1 |  |
| 2 |  |
| 9 | Temperature warning | 0 | Cancel the alarm |
| 1 |  |
| 2 |  |
| 10 | Tsunami warning | 0 | Cancel the alarm |
| 1 |  |
| 11 | Heat index | 0 | Cancel the alarm |
| 1 |  |
| 2 |  |
| 3 |  |

Example：

bd bd bd bd cb 01 01 03 dd

01 A total of 1 set of weather warning

01 SStrong Wind Signal No.3

BDBDBDBD CB 0A 0101 0201 0301 0401 0501 0601 0701 0801 0901 0A01 F5

10 sets of weather warning; note that each group of weather warning must be different, not the same type of warning, otherwise it is invalid

### 4.1.8Personal information issued（0xCA）

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_HRD\_DATA | | | |
| Decription | Server =>Terminal | | | |
| Firmware | -/- | | | |
| Payload Length | 5 bytes | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0xCA | See below | CK\_sum |

payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Byte size | Format | Name | Scale | Unit | Decription |
| 1 | U8 | count | -/- |  | Issue a few groups of information |
| 1 | U8 | type | -/- |  | type |
| 1 | U8 | len | -/- |  | length |
| N | U8 | content | -/- |  | Content (unicode coding, small end representation) |

Type:

1 – name 2 – English name 3 – phone 4 – blood type

Example：

bd bd bd bd CA 04 01 06 0B7A 2759 8765 02 18 4300 6800 6100 6e00 2000 5400 6100 6900 2000 4d00 6100 6e00

03 10 3900 3900 3800 3800 3600 3600 3300 3300 04 02 4100 dd

01 name

06 The length of 6

0B7A 2759 8765 Cheng Dawen

02 English name

18 The length of 24

4300 6800 6100 6e00 2000 5400 6100 6900 2000 4d00 6100 6e00 Chan Tai Man

03 phone number

10 The length of16

3900 3900 3800 3800 3600 3600 3300 3300 99886633

04 blood type

02 The length of2

4100 A

### 4.1.9 Issue SOS prompt message (MSGID = 0 X 80) - -universal version firmware is not available, special firmware support

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_SOS\_ DATA | | | |
| Decription | Downlink SOS message | | | |
| Firmware | -/- | | | |
| Payload Length | 4+n bytes | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0x80 | See below | CK\_sum |

payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Byte offset | Format | Name | Scale | Unit | Decription |
| 1 | U8 | length | -/- |  | contention length |
| N | N\*U8 | Content | -/- |  | Content- -unicode encoding, up to 50 words |

Example：

bd bd bd bd 80 10 5300 4F00 5300 A562 668B F25D D153 FA51dd

CONTENT LEN: 16 (0x10)

CONTENT : 5300 4F00 5300 A562 668B F25D D153 FA51 ( The SOS alarm is issued)

Applicable scenario: When a user encounters an emergency situation and triggers the SOS, the content displayed on the SOS interface can be used to take corresponding actions based on the prompts on the SOS interface

### 4.1.10 Issue message cleaning time (MSGID = 0 X 2 A) - -universal version firmware is not available, special firmware support

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_CLEANUP\_ DATA | | | |
| Decription | Downlink message cleaning time | | | |
| Firmware | -/- | | | |
| Payload Length | 4+n bytes | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0x2A | See below | CK\_sum |

payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Byte offset | Format | Name | Scale | Unit | Decription |
| 1 | U8 | hours | -/- |  | Message cleaning time (unit: hours) |

Example：

bd bd bd bd 2A 02 dd

Message cleaning time is 2 hours

### 4.1.11Set the reporting period of health data sampling（MSGID=0X1C）

The platform will set 1 to 4 times to the terminal. After the terminal, the data within the specified period

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_NB\_SLT | | | |
| Decription | down | | | |
| Firmware | -/- | | | |
| Payload Length | 28 bytes | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0x1C | See below | CK\_sum |

payload contents

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Byte offset** | **Format** | **Name** | **Scale** | **Unit** | **Decription** |  |
| 1 | u8 | enable | -/- | -/- | Enabled? | Time Slot 1 |
| 1 | U16 | Interval |  |  | Time interval (minutes) |
| 1 | u8 | time\_start\_h |  |  | -h |
| 1 | u8 | time\_start\_m |  |  | -m |
| 1 | u8 | time\_end\_h |  |  | -h |
| 1 | u8 | time\_end\_m |  |  | -m |
| 1 | u8 | enable | -/- | -/- | Enabled? | Time Slot 2 |
| 1 | U16 | Interval |  |  | Time interval (minutes) |
| 1 | u8 | time\_start\_h |  |  | -h |
| 1 | u8 | time\_start\_m |  |  | -m |
| 1 | u8 | time\_end\_h |  |  | -h |
| 1 | u8 | time\_end\_m |  |  | -m |
| 1 | u8 | enable | -/- | -/- | Enabled? | Time Slot 3 |
| 1 | U16 | Interval |  |  | Time interval (minutes) |
| 1 | u8 | time\_start\_h |  |  | -h |
| 1 | u8 | time\_start\_m |  |  | -m |
| 1 | u8 | time\_end\_h |  |  | -h |
| 1 | u8 | time\_end\_m |  |  | -n |
| 1 | u8 | enable | -/- | -/- | Enabled? | Time Slot 4 |
| 1 | U16 | Interval |  |  | Time interval (minutes) |
| 1 | u8 | time\_start\_h |  |  | -h |
| 1 | u8 | time\_start\_m |  |  | -m |
| 1 | u8 | time\_end\_h |  |  | -h |
| 1 | u8 | time\_end\_m |  |  | -m |

eg：

BDBDBDBD 1C 01 03 00 00 00 13 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 dd

From 00 to 00, heart rate, blood pressure and oxygen temperature data were reported every 3 minutes at 19

BDBDBDBD 1C 010A000000173B00000000000000000000000000000000000000000097

0-23:59, sample health data were reported at 10 minute intervals

Note: After setting, report according to the time period, and do not report outside the time period

### 4.1.12restore factory setting（MSGID=0X7B）

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Message | MSG\_RST | | | |
| Decription | restore factory setting | | | |
| Firmware | -/- | | | |
| Payload Length | 1 bytes | | | |
| Message structure | Hearer | Message ID | Payload | Checksum |
| token | 0x7B | See below | CK\_sum |

payload contents

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Byte offset | Format | Name | Scale | Unit | Decription |
| 1 | u8 | reset | -/- | -/- | 1restore factory setting |

Eg:BDBDBDBD7B018F //The device will restart after the distribution

Default general version firmware: 10 minutes location report (all day), 10 minutes sampling data report (all day), open drop alarm, open sedentary stay alarm, The default trigger time of stay alarm is 5 minutes, and the positioning priority is Bluetooth location> wifi location> gps location; text message is empty, personal information is empty; Bluetooth broadcast is enabled and data report is enabled